# Cryomodule 2K operation

The MKS2 regulation on/off is controlled by the bit m141.0 from the CM PLC.

The MKS2 PID SP is defined by the sequence parameter on HNOSS PLC (pv: CstatH-Ctrl:SQ9:cP\_CM\_SP\_MKS2) (alias CM-Ctrl:S8:cP\_SP\_PT01)

1. **Step4** – Cool down the 2K transfer line going through HX01
   1. Open CV01 to 5 %
   2. Open slowly (2% /min) CV01 to the value defined by S8\_P\_CV01
   3. Wait until CM-CM:TT02 goes below10K then goto Step6
2. **Step6** – 2K sequence on HNOSS
   1. Start the 2K operation sequence on HNOSS
   2. Close CV02
   3. Set CV01 to S8\_P\_CV01 and then turn on PID on CV01(LT01 level) when LT01 >= LT01\_Trig
   4. Wait until SQ9 on HNOSS reaches step 30 then goto Step8
3. **Step8** – Proceed to S6 (4K operation)
   1. Stop SQ9 on HNOSS

## Sequence parameters

* S8\_P\_CV01 – the final setting for step 4; the initial setting for step6
* Parameters on HNOSS for SQ9:
  + Final pressure (threshold for transition from state 14 to 16) of CM-CM:PT02 (CstatH-LHe:PT101)
  + Set-point for the 2K tank pressure PID
  + Table for control of CV551 while pumping down

## Data exchange needed between different systems

* State of SQ9 on HNOSS (from HNOSS PLC to CM PLC)

Green text – already implemented