# Cryomodule 2K operation

The MKS2 regulation on/off is controlled by the bit m141.0 from the CM PLC.

The MKS2 PID SP is defined by the sequence parameter on HNOSS PLC (pv: CstatH-Ctrl:SQ9:cP\_CM\_SP\_MKS2) (alias CM-Ctrl:S8:cP\_SP\_PT01)