# Cryomodule 4K operation

The MKS2 regulation on/off iscontrolledby the bit m141.0 fromtheCM PLC.

The MKS2 PID SP is definedby the sequence parameter on HNOSS PLC (pv: CstatH-Ctrl:SQ8:cP\_CM\_SP\_MKS2)