# Thermal screen cooling (S4)

CV60 is controlled by the PID regulator

CV61 is set to 75%.

When TT77 drops below 110 K it’s possible to proceed to LHe cooling (S5).

## Sequence parameters:

* None right now. If necessary, we can ad opening of CV60 as a parameter.

## Data exchange needed between different systems:

None.